Terrain preparation workflow in Grasshopper

Jumping dams

1. Download the data from SwissAlti3D dataset (xyz 2m): <https://www.swisstopo.admin.ch/fr/geodata/height/alti3d.html>
2. Open 1.JD\_SwissALTI3D.gh document and follow instructions inside.
3. Save DEM in the rhino document that it will be used to produce the dams.