Levels preparation workflow in Grasshopper

Jumping dams

1. This workflow requires to have the nurb terrain data into a layer called “Terrain\_brep”
2. Open 2.JD\_setup.gh document and follow instructions inside. Be aware of the data dam. It might be a bit slow.
3. Save the levels and base brep in the rhino document that it will be used to produce the dams.